Connection setup on unlocked Mio (based on Stopword):

1) Device has to be unlocked – I used  MioPocket.

2) Activate Bluetooth, but do not engage it. Make everything possible on your BT cell phone to make Mio trusted.

3) Prepare Keyboard application for later input
4) Start Control Panel and then “Network and Dial-up Connections” -> “Make New Connection”

5) Leave “Dial-Up” and press Next
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6) Press Bluetooth and then “Scan Device” (cell phone Bluetooth should be on and “trusting” ().
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7) Select entry with Phone-like icon on the left and press “->”. Reply Yes on auth dialog and enter any combination (like 111) to be repeated on cell phone.
8) Double click entry on the right to make it Active
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9) Then your Cell phone Modem becomes available and should be selected. Press «Configure”, select “Call options” tab and in “Extra settings” field type +cgdcont=1,"IP","internet" then press “ОК” and «NEXT»
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10) Erase contents of 2 upper fields (as on illustration) and in «Phone number” field type *99***1# and press “Finish”
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11) Then you have to find “Dialing Patterns” dialog and put “G” into all 3 fields as on picture.
12) Then your connection cal be activated.
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